**Changes made by Ali Ghavampour, 2022**

:S626sManager.h – Line 52

unsigned int S626sManager::readDIO(int channel, int board);

to

unsigned int readDIO(int channel, int board);

:S626sManager.cpp – Line 87

if(inputFile ==0)

to

if(inputFile.fail())

:S626sManager.cpp – Line 356

if (numAD>0)

to

if (numAD[b]>0)

:StimulatorBox.cpp – Line 128

if(inputFile ==0)

to

if(inputFile.fail())

:StimulatorBox.cpp – Line 207

if(inputFile ==0)

to

if(inputFile.fail())